LOAD PROFILING METHODOLOGY CONSULTATION

PROCEDURE CONSULTATION

SECOND STAGE PARTICIPANT RESPONSE TEMPLATE

***Participant****:*

***Submission Date****:*

Table of Contents

[1. Context 3](#_Toc119658760)

[2. Question on Load Profiling Methodology Implementation Date 3](#_Toc119658761)

[3. Metrology Procedure Part B 4](#_Toc119658762)

[4. MSATS – MDM Procedure 5](#_Toc119658763)

[5. MSATS Procedures: CATS Procedure Principles and Obligations 5](#_Toc119658764)

[6. MSATS Procedures: Procedure for the Management of Wholesale, Interconnector, Generator and Sample (WIGS) NMIs 7](#_Toc119658765)

[7. Standing Data for MSATS 8](#_Toc119658766)

[8. Retail Electricity Market Procedures – Glossary and Framework 9](#_Toc119658767)

# Context

This template is to assist stakeholders in giving feedback about the changes detailed in the draft procedures associated with the Load Profiling Methodology consultation.

The changes being proposed are due to an issue identified where negative load profiling values were present requiring changes to AEMO’s Retail Electricity Market Procedures and the following proposed changes by proponents and AEMO to implement recommended process improvements.

# Question on Load Profiling Methodology Implementation Date

| **Heading** | **Participant Comments** |
| --- | --- |
| Do you agree with AEMO’s proposed implementation date of 1 October 2023? If not, why? |  |

# Metrology Procedure Part B

|  |  |  |
| --- | --- | --- |
| **Section** | **Description** | **Participant Comments** |
| 12.4 Applying the five-minute profile positive values to 15-minute and 30-minute metering data for a Profile Area | Edited to include the new Option 6 Load Profiling Methodology |  |
| 12.5. Converting 15-minute and 30-minute metering data for a Profile Area when five-minute profile values are negative – uniform allocation method | Addition of the new Option 6 Load Profiling Methodology |  |

# MSATS – MDM Procedure

|  |  |  |
| --- | --- | --- |
| **Section** | **Description** | **Participant Comments** |
| 3.2.3 Characteristics of the 5MLP | Addition of reference to section 12.5 Metrology Procedure: Part B |  |
| 9.16 MDM-RM46 | Update of description of the RM46 Report |  |

# MSATS Procedures: CATS Procedure Principles and Obligations

|  |  |  |
| --- | --- | --- |
| **Section** | **Description** | **Participant Comments** |
| 4.12 Embedded Network Codes and Rules | Addition of:  (iv) once all obligations have been met under the NER Chapter 5 and 5A and jurisdictional documentation, the LNSP must provide the Embedded Network Code to AEMO within five business days from the time it receives the request from the embedded network owner or the ENM acting on behalf of the embedded network owner, where the site is:   1. a Greenfield Site; 2. a Brownfield Site that for all intents and purposes has been set up as an embedded network but all consumers were purchasing energy from the embedded network owner; and 3. a Brownfield Site that may require network infrastructure changes. |  |
| 9.1.4 LNSP Requirements | Addition of House Number To Suffix in ( e) |  |
| 9.2.4 ENM Requirements | Addition of House Number To Suffix in ( e) |  |
| 9.3.4 LNSP Requirements | Addition of House Number To Suffix in (f) |  |
| 9.4.4 ENM Requirements | Addition of House Number To Suffix in (g) |  |
| 12.2.4 LNSP Requirements (5001 only) | Addition of House Number To Suffix in (d) |  |
| 12.2.4 ENM Requirements (5021 only) | Addition of House Number To Suffix in (c) |  |
| 12.3.4 LNSP Requirements | Addition of House Number To Suffix in (d) |  |
| 12.6.4 ENM Requirements | Addition of House Number To Suffix in (d) |  |
| 15.1.4 AEMO Requirements | Addition of House Number To Suffix in (d) |  |
| Table 16-C – NMI Standing Data Items and CATS Standing Data NMI Discovery Data Access Rules | Addition of HouseNumToSuffix |  |

# MSATS Procedures: Procedure for the Management of Wholesale, Interconnector, Generator and Sample (WIGS) NMIs

|  |  |  |
| --- | --- | --- |
| **Section** | **Description** | **Participant Comments** |
| 4.1.4 LNSP Requirements | Addition of House Number To Suffix in ( e) |  |
| 4.2.4 ENM Requirements | Addition of House Number To Suffix in ( e) |  |
| 4.3.4 LNSP Requirements | Addition of House Number To Suffix in (f) |  |
| 7.1.4 LNSP Requirements | Addition of House Number To Suffix in (d) |  |
| 7.1.5 ENM Requirements (5021 only) | Addition of House Number To Suffix in (d) |  |
| 7.2.3 LNSP Requirements | Addition of House Number To Suffix in (d) |  |
| 7.4.4 ENM Requirements | Addition of House Number To Suffix in (d) |  |
| 9.1.4 AEMO Requirements | Addition of House Number To Suffix in (b) |  |

# Standing Data for MSATS

|  |  |  |
| --- | --- | --- |
| **Section** | **Description** | **Participant Comments** |
| Table 12 CATS\_NMI\_DATA – Field Definitions | Addition of Data Element Name HouseNumberToSuffix |  |
| Table 13 CATS\_NMI\_Data | Addition of House Number To Suffix |  |
| Table 14 CATS\_NMI\_Data Field value examples | Addition of HouseNumberToSuffix |  |

# Retail Electricity Market Procedures – Glossary and Framework

|  |  |  |
| --- | --- | --- |
| **Section** | **Description** | **Participant Comments** |
| 5. Glossary | Addition of the definition of LCCD |  |
|  |  |  |
|  |  |  |